<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;"># See $ANALYZER/examples/output_example.def for examples
#
block T.shms.*
block P.ngcer.*
block P.dc.*
block P.tr.*
block P.hod.*
block P.hgcer.*
block P.aero.*
block P.cal.*
#block P.gtr.*

# Noble Gas Cherenkov
TH1F pngcer_occu 'SHMS Noble Gas Cherenkov Occupancy; Counter Number; Number of Entries' P.ngcer.adcCounter 4 0.5 4.5
TH2F pngcer_ped_vs_cntr 'SHMS Noble Gas Cherenkov Pulse Pedestal vs. Counter Number; Counter Number;  Pulse Pedestal / 1 ADC Unit' P.ngcer.adcCounter P.ngcer.adcPed 4 0.5 4.5 1000 0 1000
TH2F pngcer_pi_vs_cntr 'SHMS Noble Gas Cherenkov Pulse Integral vs. Counter Number; Counter Number;  Pulse Integral / 10 ADC Units' P.ngcer.adcCounter P.ngcer.adcPulseInt 4 0.5 4.5 4000 0 40000
TH2F pngcer_amp_vs_cntr 'SHMS Noble Gas Cherenkov Pulse Amplitude vs. Counter Number; Counter Number;  Pulse Amplitude / 1 ADC Unit' P.ngcer.adcCounter P.ngcer.adcPulseAmp 4 0.5 4.5 4100 0 4100

# Drift Chambers
TH1F pdc_ref1  'SHMS DC Reference Time Slot 6 Channel 79; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF1_tdcTime  200 12000 14000
TH1F pdc_ref2  'SHMS DC Reference Time Slot 7 Channel 79; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF2_tdcTime  200 12000 14000
TH1F pdc_ref3  'SHMS DC Reference Time Slot 8 Channel 79; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF3_tdcTime  200 12000 14000
TH1F pdc_ref4  'SHMS DC Reference Time Slot 9 Channel 79; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF4_tdcTime  200 12000 14000
TH1F pdc_ref5  'SHMS DC Reference Time Slot 10 Channel 79; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF5_tdcTime  200 12000 14000
TH1F pdc_ref6  'SHMS DC Reference Time Slot 11 Channel 47; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF6_tdcTime  200 12000 14000
TH1F pdc_ref7  'SHMS DC Reference Time Slot 12 Channel 47; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF7_tdcTime  200 12000 14000
TH1F pdc_ref8  'SHMS DC Reference Time Slot 13 Channel 47; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF8_tdcTime  200 12000 14000
TH1F pdc_ref9  'SHMS DC Reference Time Slot 14 Channel 15; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF9_tdcTime  200 12000 14000
TH1F pdc_ref10 'SHMS DC Reference Time Slot 15 Channel 47; Raw TDC Time (TDC Clicks); Counts / 10 TDC Clicks;' T.shms.pDCREF10_tdcTime 200 12000 14000

TH1F pdc1u1_wirenum 'SHMS DC 1U1 Wiremap; Wire Number; Number of Entries' P.dc.1u1.wirenum 107 0.5 107.5
TH1F pdc1u2_wirenum 'SHMS DC 1U2 Wiremap; Wire Number; Number of Entries' P.dc.1u2.wirenum 107 0.5 107.5
TH1F pdc1x1_wirenum 'SHMS DC 1X1 Wiremap; Wire Number; Number of Entries' P.dc.1x1.wirenum  79 0.5  79.5
TH1F pdc1x2_wirenum 'SHMS DC 1X2 Wiremap; Wire Number; Number of Entries' P.dc.1x2.wirenum  79 0.5  79.5
TH1F pdc1v1_wirenum 'SHMS DC 1V1 Wiremap; Wire Number; Number of Entries' P.dc.1v1.wirenum 107 0.5 107.5
TH1F pdc1v2_wirenum 'SHMS DC 1V2 Wiremap; Wire Number; Number of Entries' P.dc.1v2.wirenum 107 0.5 107.5

TH1F pdc2v2_wirenum 'SHMS DC 2V2 Wiremap; Wire Number; Number of Entries' P.dc.2v2.wirenum 107 0.5 107.5
TH1F pdc2v1_wirenum 'SHMS DC 2V1 Wiremap; Wire Number; Number of Entries' P.dc.2v1.wirenum 107 0.5 107.5
TH1F pdc2x2_wirenum 'SHMS DC 2X2 Wiremap; Wire Number; Number of Entries' P.dc.2x2.wirenum  79 0.5  79.5
TH1F pdc2x1_wirenum 'SHMS DC 2X1 Wiremap; Wire Number; Number of Entries' P.dc.2x1.wirenum  79 0.5  79.5
TH1F pdc2u2_wirenum 'SHMS DC 2U2 Wiremap; Wire Number; Number of Entries' P.dc.2u2.wirenum 107 0.5 107.5
TH1F pdc2u1_wirenum 'SHMS DC 2U1 Wiremap; Wire Number; Number of Entries' P.dc.2u1.wirenum 107 0.5 107.5

TH2F pdc1u1_wirenum_vs_tdc 'SHMS DC 1U1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1u1.wirenum P.dc.1u1.time 107 0.5 107.5 600 -100 500
TH2F pdc1u2_wirenum_vs_tdc 'SHMS DC 1U2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1u2.wirenum P.dc.1u2.time 107 0.5 107.5 600 -100 500
TH2F pdc1x1_wirenum_vs_tdc 'SHMS DC 1X1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1x1.wirenum P.dc.1x1.time  79 0.5  79.5 600 -100 500
TH2F pdc1x2_wirenum_vs_tdc 'SHMS DC 1X2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1x2.wirenum P.dc.1x2.time  79 0.5  79.5 600 -100 500
TH2F pdc1v1_wirenum_vs_tdc 'SHMS DC 1V1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1v1.wirenum P.dc.1v1.time 107 0.5 107.5 600 -100 500
TH2F pdc1v2_wirenum_vs_tdc 'SHMS DC 1V2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.1v2.wirenum P.dc.1v2.time 107 0.5 107.5 600 -100 500

TH2F pdc2v2_wirenum_vs_tdc 'SHMS DC 2V2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2v2.wirenum P.dc.2v2.time 107 0.5 107.5 600 -100 500
TH2F pdc2v1_wirenum_vs_tdc 'SHMS DC 2V1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2v1.wirenum P.dc.2v1.time 107 0.5 107.5 600 -100 500
TH2F pdc2x2_wirenum_vs_tdc 'SHMS DC 2X2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2x2.wirenum P.dc.2x2.time  79 0.5  79.5 600 -100 500
TH2F pdc2x1_wirenum_vs_tdc 'SHMS DC 2X1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2x1.wirenum P.dc.2x1.time  79 0.5  79.5 600 -100 500
TH2F pdc2u2_wirenum_vs_tdc 'SHMS DC 2U2 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2u2.wirenum P.dc.2u2.time 107 0.5 107.5 600 -100 500
TH2F pdc2u1_wirenum_vs_tdc 'SHMS DC 2U1 Wire Number vs. TDC; Wire Number; TDC Time (ns) / 1 ns' P.dc.2u1.wirenum P.dc.2u1.time 107 0.5 107.5 600 -100 500

TH2F pdc1u1_wirenum_vs_ddist 'SHMS 1U1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1u1.wirenum P.dc.1u1.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc1u2_wirenum_vs_ddist 'SHMS 1U2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1u2.wirenum P.dc.1u2.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc1x1_wirenum_vs_ddist 'SHMS 1X1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1x1.wirenum P.dc.1x1.dist  79 0.5  79.5 300 -0.1 0.6
TH2F pdc1x2_wirenum_vs_ddist 'SHMS 1X2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1x2.wirenum P.dc.1x2.dist  79 0.5  79.5 300 -0.1 0.6
TH2F pdc1v1_wirenum_vs_ddist 'SHMS 1V1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1v1.wirenum P.dc.1v1.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc1v2_wirenum_vs_ddist 'SHMS 1V2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.1v2.wirenum P.dc.1v2.dist 107 0.5 107.5 300 -0.1 0.6

TH2F pdc2u2_wirenum_vs_ddist 'SHMS 2U2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2u2.wirenum P.dc.2u2.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc2u1_wirenum_vs_ddist 'SHMS 2U1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2u1.wirenum P.dc.2u1.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc2x2_wirenum_vs_ddist 'SHMS 2X2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2x2.wirenum P.dc.2x2.dist  79 0.5  79.5 300 -0.1 0.6
TH2F pdc2x1_wirenum_vs_ddist 'SHMS 2X1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2x1.wirenum P.dc.2x1.dist  79 0.5  79.5 300 -0.1 0.6
TH2F pdc2v2_wirenum_vs_ddist 'SHMS 2V2 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2v2.wirenum P.dc.2v2.dist 107 0.5 107.5 300 -0.1 0.6
TH2F pdc2v1_wirenum_vs_ddist 'SHMS 2V1 Wire Number vs. Drift Distance; Wire Number; Drift Distance (cm)' P.dc.2v1.wirenum P.dc.2v1.dist 107 0.5 107.5 300 -0.1 0.6

TH2F pdc1u1_wirenum_vs_resid 'SHMS 1U1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1u1.wirenum P.dc.residual[0] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc1u2_wirenum_vs_resid 'SHMS 1U2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1u2.wirenum P.dc.residual[1] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc1x1_wirenum_vs_resid 'SHMS 1X1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1x1.wirenum P.dc.residual[2] 79 0.5  79.5 200 -1.0 1.0
TH2F pdc1x2_wirenum_vs_resid 'SHMS 1X2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1x2.wirenum P.dc.residual[3] 79 0.5  79.5 200 -1.0 1.0
TH2F pdc1v1_wirenum_vs_resid 'SHMS 1V1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1v1.wirenum P.dc.residual[4] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc1v2_wirenum_vs_resid 'SHMS 1V2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.1v2.wirenum P.dc.residual[5] 107 0.5 107.5 200 -1.0 1.0

TH2F pdc2v2_wirenum_vs_resid 'SHMS 2V2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2v2.wirenum P.dc.residual[6] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc2v1_wirenum_vs_resid 'SHMS 2V1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2v1.wirenum P.dc.residual[7] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc2x2_wirenum_vs_resid 'SHMS 2X2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2x2.wirenum P.dc.residual[8] 79 0.5  79.5 200 -1.0 1.0
TH2F pdc2x1_wirenum_vs_resid 'SHMS 2X1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2x1.wirenum P.dc.residual[9] 79 0.5  79.5 200 -1.0 1.0
TH2F pdc2u2_wirenum_vs_resid 'SHMS 2U2 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2u2.wirenum P.dc.residual[10] 107 0.5 107.5 200 -1.0 1.0
TH2F pdc2u1_wirenum_vs_resid 'SHMS 2U1 DC Wire Number vs. Residuals; Wire Number; Residuals (cm)' P.dc.2u1.wirenum P.dc.residual[11] 107 0.5 107.5 200 -1.0 1.0

TH2F pdc_xfp_vs_yxp 'SHMS DC Xfp vs Yxp; Yfp (cm) / 1 cm; Xfp (cm) / 1 cm' P.dc.y P.dc.x 100 -50 50 100 -50 50
TH2F pdc_xfpp_vs_yxpp 'SHMS DC Xfpp vs Yxpp; Yfpp; Xfpp' P.dc.yp P.dc.xp 100 -1 1 100 -1 1

# Hodoscopes (Positive/Left) 
TH1F phodo_1x_pos_adc_occu 'SHMS Hodoscope 1X+ ADC Occupancy; Paddle Number; Number of Hits' P.hod.1x.posAdcCounter 13 0.5 13.5
TH1F phodo_1y_pos_adc_occu 'SHMS Hodoscope 1Y+ ADC Occupancy; Paddle Number; Number of Hits' P.hod.1y.posAdcCounter 13 0.5 13.5 
TH1F phodo_2x_pos_adc_occu 'SHMS Hodoscope 2X+ ADC Occupancy; Paddle Number; Number of Hits' P.hod.2x.posAdcCounter 14 0.5 14.5
TH1F phodo_2y_pos_adc_occu 'SHMS Hodoscope 2Y+ ADC Occupancy; Paddle Number; Number of Hits' P.hod.2y.posAdcCounter 21 0.5 21.5
TH1F phodo_1x_pos_tdc_occu 'SHMS Hodoscope 1X+ TDC Occupancy; Paddle Number; Number of Hits' P.hod.1x.posTdcCounter 13 0.5 13.5
TH1F phodo_1y_pos_tdc_occu 'SHMS Hodoscope 1Y+ TDC Occupancy; Paddle Number; Number of Hits' P.hod.1y.posTdcCounter 13 0.5 13.5 
TH1F phodo_2x_pos_tdc_occu 'SHMS Hodoscope 2X+ TDC Occupancy; Paddle Number; Number of Hits' P.hod.2x.posTdcCounter 14 0.5 14.5
TH1F phodo_2y_pos_tdc_occu 'SHMS Hodoscope 2Y+ TDC Occupancy; Paddle Number; Number of Hits' P.hod.2y.posTdcCounter 21 0.5 21.5
TH2F phodo_1x_pos_ped_vs_pad 'SHMS Hodoscope 1X+ Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.1x.posAdcCounter  P.hod.1x.posAdcPed 13 0.5 13.5 1000 0 1000
TH2F phodo_1y_pos_ped_vs_pad 'SHMS Hodoscope 1Y+ Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.1y.posAdcCounter  P.hod.1y.posAdcPed 13 0.5 13.5 1000 0 1000
TH2F phodo_2x_pos_ped_vs_pad 'SHMS Hodoscope 2X+ Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.2x.posAdcCounter  P.hod.2x.posAdcPed 14 0.5 14.5 1000 0 1000
TH2F phodo_2y_pos_ped_vs_pad 'SHMS Hodoscope 2Y+ Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.2y.posAdcCounter  P.hod.2y.posAdcPed 21 0.5 21.5 1000 0 1000
TH2F phodo_1x_pos_pi_vs_pad 'SHMS Hodoscope 1X+ Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.1x.GoodPaddle  P.hod.1x.GoodPosAdcPulseInt 13 0.5 13.5 4000 0 40000
TH2F phodo_1y_pos_pi_vs_pad 'SHMS Hodoscope 1Y+ Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.1y.GoodPaddle  P.hod.1y.GoodPosAdcPulseInt 13 0.5 13.5 4000 0 40000
TH2F phodo_2x_pos_pi_vs_pad 'SHMS Hodoscope 2X+ Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.2x.GoodPaddle  P.hod.2x.GoodPosAdcPulseInt 14 0.5 14.5 4000 0 40000
TH2F phodo_2y_pos_pi_vs_pad 'SHMS Hodoscope 2Y+ Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.2y.GoodPaddle  P.hod.2y.GoodPosAdcPulseInt 21 0.5 21.5 4000 0 40000
TH2F phodo_1x_pos_pamp_vs_pad 'SHMS Hodoscope 1X+ Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.1x.GoodPaddle  P.hod.1x.GoodPosAdcPulseAmp 13 0.5 13.5 4100 0 4100
TH2F phodo_1y_pos_pamp_vs_pad 'SHMS Hodoscope 1Y+ Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.1y.GoodPaddle  P.hod.1y.GoodPosAdcPulseAmp 13 0.5 13.5 4100 0 4100
TH2F phodo_2x_pos_pamp_vs_pad 'SHMS Hodoscope 2X+ Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.2x.GoodPaddle  P.hod.2x.GoodPosAdcPulseAmp 14 0.5 14.5 4100 0 4100
TH2F phodo_2y_pos_pamp_vs_pad 'SHMS Hodoscope 2Y+ Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.2y.GoodPaddle  P.hod.2y.GoodPosAdcPulseAmp 21 0.5 21.5 4100 0 4100
TH2F phodo_1x_pos_tdc_time_vs_pad 'SHMS Hodoscope 1X+ TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.1x.GoodPaddle  P.hod.1x.GoodPosTdcChan 13 0.5 13.5 3500 -500 3000
TH2F phodo_1y_pos_tdc_time_vs_pad 'SHMS Hodoscope 1Y+ TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.1y.GoodPaddle  P.hod.1y.GoodPosTdcChan 13 0.5 13.5 3500 -500 3000
TH2F phodo_2x_pos_tdc_time_vs_pad 'SHMS Hodoscope 2X+ TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.2x.GoodPaddle  P.hod.2x.GoodPosTdcChan 14 0.5 14.5 3500 -500 3000
TH2F phodo_2y_pos_tdc_time_vs_pad 'SHMS Hodoscope 2Y+ TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.2y.GoodPaddle  P.hod.2y.GoodPosTdcChan 21 0.5 21.5 3500 -500 3000

# Hodoscopes (Negative/Right)
TH1F phodo_1x_neg_adc_occu 'SHMS Hodoscope 1X- ADC Occupancy; Paddle Number; Number of Hits' P.hod.1x.negAdcCounter 13 0.5 13.5
TH1F phodo_1y_neg_adc_occu 'SHMS Hodoscope 1Y- ADC Occupancy; Paddle Number; Number of Hits' P.hod.1y.negAdcCounter 13 0.5 13.5 
TH1F phodo_2x_neg_adc_occu 'SHMS Hodoscope 2X- ADC Occupancy; Paddle Number; Number of Hits' P.hod.2x.negAdcCounter 14 0.5 14.5
TH1F phodo_2y_neg_adc_occu 'SHMS Hodoscope 2Y- ADC Occupancy; Paddle Number; Number of Hits' P.hod.2y.negAdcCounter 21 0.5 21.5
TH1F phodo_1x_neg_tdc_occu 'SHMS Hodoscope 1X- TDC Occupancy; Paddle Number; Number of Hits' P.hod.1x.negTdcCounter 13 0.5 13.5
TH1F phodo_1y_neg_tdc_occu 'SHMS Hodoscope 1Y- TDC Occupancy; Paddle Number; Number of Hits' P.hod.1y.negTdcCounter 13 0.5 13.5 
TH1F phodo_2x_neg_tdc_occu 'SHMS Hodoscope 2X- TDC Occupancy; Paddle Number; Number of Hits' P.hod.2x.negTdcCounter 14 0.5 14.5
TH1F phodo_2y_neg_tdc_occu 'SHMS Hodoscope 2Y- TDC Occupancy; Paddle Number; Number of Hits' P.hod.2y.negTdcCounter 21 0.5 21.5
TH2F phodo_1x_neg_ped_vs_pad 'SHMS Hodoscope 1X- Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.1x.negAdcCounter  P.hod.1x.negAdcPed 13 0.5 13.5 1000 0 1000
TH2F phodo_1y_neg_ped_vs_pad 'SHMS Hodoscope 1Y- Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.1y.negAdcCounter  P.hod.1y.negAdcPed 13 0.5 13.5 1000 0 1000
TH2F phodo_2x_neg_ped_vs_pad 'SHMS Hodoscope 2X- Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.2x.negAdcCounter  P.hod.2x.negAdcPed 14 0.5 14.5 1000 0 1000
TH2F phodo_2y_neg_ped_vs_pad 'SHMS Hodoscope 2Y- Pulse Pedestal vs. Paddle Number; Paddle Number; Pulse Pedestal / 1 ADC Unit' P.hod.2y.negAdcCounter  P.hod.2y.negAdcPed 21 0.5 21.5 1000 0 1000
TH2F phodo_1x_neg_pi_vs_pad 'SHMS Hodoscope 1X- Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.1x.GoodPaddle  P.hod.1x.GoodNegAdcPulseInt 13 0.5 13.5 4000 0 40000
TH2F phodo_1y_neg_pi_vs_pad 'SHMS Hodoscope 1Y- Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.1y.GoodPaddle  P.hod.1y.GoodNegAdcPulseInt 13 0.5 13.5 4000 0 40000
TH2F phodo_2x_neg_pi_vs_pad 'SHMS Hodoscope 2X- Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.2x.GoodPaddle  P.hod.2x.GoodNegAdcPulseInt 14 0.5 14.5 4000 0 40000
TH2F phodo_2y_neg_pi_vs_pad 'SHMS Hodoscope 2Y- Pulse Integral vs. Paddle Number; Paddle Number; Pulse Integral / 10 ADC Units' P.hod.2y.GoodPaddle  P.hod.2y.GoodNegAdcPulseInt 21 0.5 21.5 4000 0 40000
TH2F phodo_1x_neg_pamp_vs_pad 'SHMS Hodoscope 1X- Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.1x.GoodPaddle  P.hod.1x.GoodNegAdcPulseAmp 13 0.5 13.5 4100 0 4100
TH2F phodo_1y_neg_pamp_vs_pad 'SHMS Hodoscope 1Y- Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.1y.GoodPaddle  P.hod.1y.GoodNegAdcPulseAmp 13 0.5 13.5 4100 0 4100
TH2F phodo_2x_neg_pamp_vs_pad 'SHMS Hodoscope 2X- Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.2x.GoodPaddle  P.hod.2x.GoodNegAdcPulseAmp 14 0.5 14.5 4100 0 4100
TH2F phodo_2y_neg_pamp_vs_pad 'SHMS Hodoscope 2Y- Pulse Amplitude vs. Paddle Number; Paddle Number; Pulse Amplitude / 1 ADC Unit' P.hod.2y.GoodPaddle  P.hod.2y.GoodNegAdcPulseAmp 21 0.5 21.5 4100 0 4100
TH2F phodo_1x_neg_tdc_time_vs_pad 'SHMS Hodoscope 1X- TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.1x.GoodPaddle  P.hod.1x.GoodNegTdcChan 13 0.5 13.5 3500 -500 3000
TH2F phodo_1y_neg_tdc_time_vs_pad 'SHMS Hodoscope 1Y- TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.1y.GoodPaddle  P.hod.1y.GoodNegTdcChan 13 0.5 13.5 3500 -500 3000
TH2F phodo_2x_neg_tdc_time_vs_pad 'SHMS Hodoscope 2X- TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.2x.GoodPaddle  P.hod.2x.GoodNegTdcChan 14 0.5 14.5 3500 -500 3000
TH2F phodo_2y_neg_tdc_time_vs_pad 'SHMS Hodoscope 2Y- TDC Time vs. Paddle Number; Paddle Number; TDC Time (ns) / 1 ns' P.hod.2y.GoodPaddle  P.hod.2y.GoodNegTdcChan 21 0.5 21.5 3500 -500 3000

# Heavy Gas Cherenkov
TH1F phgcer_occu 'SHMS Heavy Gas Cherenkov Occupancy; Counter Number; Number of Entries' P.hgcer.adcCounter 4 0.5 4.5
TH2F phgcer_ped_vs_cntr 'SHMS Heavy Gas Cherenkov Pulse Pedestal vs. Counter Number; Counter Number;  Pulse Pedestal / 1 ADC Unit' P.hgcer.adcCounter P.hgcer.adcPed 4 0.5 4.5 1000 0 1000
TH2F phgcer_pi_vs_cntr 'SHMS Heavy Gas Cherenkov Pulse Integral vs. Counter Number; Counter Number;  Pulse Integral / 10 ADC Units' P.hgcer.adcCounter P.hgcer.adcPulseInt 4 0.5 4.5 4000 0 40000
TH2F phgcer_amp_vs_cntr 'SHMS Heavy Gas Cherenkov Pulse Amplitude vs. Counter Number; Counter Number;  Pulse Amplitude / 1 ADC Unit' P.hgcer.adcCounter P.hgcer.adcPulseAmp 4 0.5 4.5 4100 0 4100

# Aerogel
TH1F paero_pos_occu 'SHMS Aero+ Occupancy; Counter Number; Number of Entries' P.aero.posAdcCounter 7 0.5 7.5
TH2F paero_pos_ped_vs_cntr 'SHMS Aero+ Pulse Pedestal vs. Counter Number; Counter Number;  Pulse Pedestal / 1 ADC Unit' P.aero.posAdcCounter P.aero.posAdcPed 7 0.5 7.5 1000 0 1000
TH2F paero_pos_pi_vs_cntr 'SHMS Aero+ Pulse Integral vs. Counter Number; Counter Number;  Pulse Integral / 10 ADC Units' P.aero.posAdcCounter P.aero.posAdcPulseInt 7 0.5 7.5 4000 0 40000
TH2F paero_pos_amp_vs_cntr 'SHMS Aero+ Pulse Amplitude vs. Counter Number; Counter Number;  Pulse Amplitude / 1 ADC Unit' P.aero.posAdcCounter P.aero.posAdcPulseAmp 7 0.5 7.5 4100 0 4100
TH1F paero_neg_occu 'SHMS Aero- Occupancy; Counter Number; Number of Entries' P.aero.negAdcCounter 7 0.5 7.5
TH2F paero_neg_ped_vs_cntr 'SHMS Aero- Pulse Pedestal vs. Counter Number; Counter Number;  Pulse Pedestal / 1 ADC Unit' P.aero.negAdcCounter P.aero.negAdcPed 7 0.5 7.5 1000 0 1000
TH2F paero_neg_pi_vs_cntr 'SHMS Aero- Pulse Integral vs. Counter Number; Counter Number;  Pulse Integral / 10 ADC Units' P.aero.negAdcCounter P.aero.negAdcPulseInt 7 0.5 7.5 4000 0 40000
TH2F paero_neg_amp_vs_cntr 'SHMS Aero- Pulse Amplitude vs. Counter Number; Counter Number;  Pulse Amplitude / 1 ADC Unit' P.aero.negAdcCounter P.aero.negAdcPulseAmp 7 0.5 7.5 4100 0 4100

# Pre-Shower Calorimeter
TH1F pcal_prshwr_pos_occu 'SHMS Preshower+ Occupancy; Block Number; Number of Entries' P.cal.pr.posAdcCounter 14 0.5 14.5
TH2F pcal_prshwr_pos_ped_blk 'SHMS Preshower+ Pulse Pedestal vs. Block Number; Block Number; Pulse Pedestal / 1 ADC Unit' P.cal.pr.posAdcCounter P.cal.pr.posAdcPed 14 0.5 14.5 1000 0 1000
TH2F pcal_prshwr_pos_pi_blk 'SHMS Preshower+ Pulse Integral vs. Block Number; Block Number; Pulse Integral / 10 ADC Units' P.cal.pr.posAdcCounter P.cal.pr.posAdcPulseInt 14 0.5 14.5 4000 0 40000
TH2F pcal_prshwr_pos_amp_blk 'SHMS Preshower+ Pulse Amplitude vs. Block Number; Block Number; Pulse Amplitude / 1 ADC Unit' P.cal.pr.posAdcCounter P.cal.pr.posAdcPulseAmp 14 0.5 14.5 4100 0 4100
TH1F pcal_prshwr_neg_occu 'SHMS Preshower- Occupancy; Block Number; Number of Entries' P.cal.pr.negAdcCounter 14 0.5 14.5
TH2F pcal_prshwr_neg_ped_blk 'SHMS Preshower- Pulse Pedestal vs. Block Number; Block Number; Pulse Pedestal / 1 ADC Unit' P.cal.pr.negAdcCounter P.cal.pr.negAdcPed 14 0.5 14.5 1000 0 1000
TH2F pcal_prshwr_neg_pi_blk 'SHMS Preshower- Pulse Integral vs. Block Number; Block Number; Pulse Integral / 10 ADC Units' P.cal.pr.negAdcCounter P.cal.pr.negAdcPulseInt 14 0.5 14.5 4000 0 40000
TH2F pcal_prshwr_neg_amp_blk 'SHMS Preshower- Pulse Amplitude vs. Block Number; Block Number; Pulse Amplitude / 1 ADC Unit' P.cal.pr.negAdcCounter P.cal.pr.negAdcPulseAmp 14 0.5 14.5 4100 0 4100 

# Shower Calorimeter
TH1F pcal_shwr_occu 'SHMS Shower Occupancy; Block Number; Number of Entries' P.cal.fly.adcCounter 224 0.5 224.5
TH2F pcal_shwr_ped_blk 'SHMS Shower Pulse Pedestal vs. Block Number; Block Number; Pulse Pedestal / 1 ADC Unit' P.cal.fly.adcCounter P.cal.fly.adcPed 224 0.5 224.5 1000 0 1000
TH2F pcal_shwr_pi_blk 'SHMS Shower Pulse Integral vs. Block Number; Block Number; Pulse Integral / 10 ADC Units' P.cal.fly.adcCounter P.cal.fly.adcPulseInt 224 0.5 224.5 4000 0 40000
TH2F pcal_shwr_amp_blk 'SHMS Shower Pulse Amplitude vs. Block Number; Block Number; Pulse Amplitude / 1 ADC Unit' P.cal.fly.adcCounter P.cal.fly.adcPulseAmp 224 0.5 224.5 4100 0 4100 

# Trigger Apparatus
TH1F ptrig_pngc_sum_pped 'SHMS Noble Gas Sum FADC Pulse Pedestal; Pulse Pedestal; Number of Entries / 1 ADC Units' T.shms.pNGCSUM_adcPed 2000 0 2000
TH1F ptrig_pngc_sum_pint 'SHMS Noble Gas Sum FADC Pulse Integral; Pulse Integral; Number of Entries / 10 ADC Units' T.shms.pNGCSUM_adcPulseInt 4000 0 40000
TH1F ptrig_pngc_sum_pamp 'SHMS Noble Gas Sum FADC Pulse Amplitude; Pulse Amplitude; Number of Entries / 1 ADC Units' T.shms.pNGCSUM_adcPulseAmp 4100 0 4100
TH1F ptrig_pngc_sum_ptime 'SHMS Noble Gas Sum FADC Pulse Time; Pulse Time; Number of Entries / 10 ADC Units' T.shms.pNGCSUM_adcPulseTimeRaw 1000 0 10000
TH1F ptrig_pngc_sum_tdc 'SHMS Noble Gas Sum TDC Time; TDC Time; Number of Entries / 10 TDC Units' T.shms.pNGCSUM_tdcTime 700 -3500 3500

TH1F ptrig_phgc_sum_pped 'SHMS Heavy Gas Sum FADC Pulse Pedestal; Pulse Pedestal; Number of Entries / 1 ADC Units' T.shms.pHGCSUM_adcPed 2000 0 2000
TH1F ptrig_phgc_sum_pint 'SHMS Heavy Gas Sum FADC Pulse Integral; Pulse Integral; Number of Entries / 10 ADC Units' T.shms.pHGCSUM_adcPulseInt 4000 0 40000
TH1F ptrig_phgc_sum_pamp 'SHMS Heavy Gas Sum FADC Pulse Amplitude; Pulse Amplitude; Number of Entries / 1 ADC Units' T.shms.pHGCSUM_adcPulseAmp 4100 0 4100
TH1F ptrig_phgc_sum_ptime 'SHMS Heavy Gas Sum FADC Pulse Time; Pulse Time; Number of Entries / 10 ADC Units' T.shms.pHGCSUM_adcPulseTimeRaw 1000 0 10000
TH1F ptrig_phgc_sum_tdc 'SHMS Heavy Gas Sum TDC Time; TDC Time; Number of Entries / 10 TDC Units' T.shms.pHGCSUM_tdcTime 700 -3500 3500

TH1F ptrig_p1x_tdc 'SHMS p1x TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p1X_tdcTime 350 0 3500
TH1F ptrig_p1y_tdc 'SHMS p1y TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p1Y_tdcTime 350 0 3500
TH1F ptrig_p2x_tdc 'SHMS p2x TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p2X_tdcTime 350 0 3500
TH1F ptrig_p2y_tdc 'SHMS p2y TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p2Y_tdcTime 350 0 3500

TH1F ptrig_p1T_tdc 'SHMS p1x/p1y Coincidence TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p1T_tdcTime 350 0 3500
TH1F ptrig_p2T_tdc 'SHMS p2x/p2y Coincidence TDC Time; Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.p2T_tdcTime 350 0 3500

TH1F ptrig_pT1_tdc 'SHMS p1x/p1y/p2x/p2y Coincidence TDC Time (Slot 20, Channel 15); Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.pT1_tdcTime 350 0 3500
TH1F ptrig_pT2_tdc 'SHMS p1x/p1y/p2x/p2y Coincidence TDC Time (Slot 19, Channel 31); Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.pT2_tdcTime 350 0 3500
TH1F ptrig_pT3_tdc 'SHMS p1x/p1y/p2x/p2y Coincidence TDC Time (Slot 19, Channel 38); Raw TDC Time (TDC Units); Counts / 10 TDC Units;' T.shms.pT3_tdcTime 350 0 3500
</pre></body></html>